Specifications
	Model
	MJ36-140
	MJ36-210
	

	Transport Width
	1.60m (5’3″)
	1.60m (5’3″)
	

	Working  Width
	1.43m (4′ 8.5″)
	2.11m (6′ 11″)
	

	Power Requirements
	70-120 HP
	90-150 HP
	

	Cutting Height
	15-100mm
	15-100mm
	

	Number of Rotors
	2
	3
	

	Number of Blades
	8
	12
	

	Sliding Offset
	1.56m
	1.56m
	

	Hedge Cutting
	0÷95°
	0÷95°
	

	Roadside mowing
	0÷35°
	0÷35°
	

	Tractor Class
	II
	II
	

	Weight
	690kg
	810kg
	

	Flow rates
	70 litre/min
	88 litre/min
	



